{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":5,"n_cols":11,"rows_kept":5,"merged":[[0,0,0,10],[3,2,3,5],[4,0,4,10]]}
["广西医科大学第二附属医院食堂智能烹饪设备采购需求表"]
["序号","名称","技术参数","品牌","型号","单位","数量","单价（元）","金额（元）","图片","商品保修期"]
[1,"AI智能烹饪柜","1.硬件参数：\n（1）盒装食物总容量：根据不同规格餐盒可容纳72-720盒。\n（2）温度隔离且独立受控的烹调格数目：18个。\n（3）具备制冷与加热系统，可实现理论值0℃—140℃的可变温度控制。\n（4）电网供电参数：\na.三相四线或三相五线。\nb.相电压380V。\nc.频率50HZ。\nd.整柜峰值功率：36KW。\ne.烹调格单元峰值功率：2KW。\nf.满负荷烹饪用电量：36度电（按整柜满载食物，从0°C加热到100°C进行核算）。\ng.制冷峰值功率：2匹。\n1.用料：采用食品级材料，具备防水防潮防锈功能。\n2.生产效率：单台机单餐次产能50kg以上，可同时烹饪10种及以上菜品、批量出餐。\n3.设备符合国标认证。\n4.设备可通过手机、电脑等移动终端进行远程控制、定时执行；远程线上监控、故障预警功能；\n5.设备配套智慧系统，可实现数字化烹饪信息展示。\n6.设备能源输入须为电能，食堂仅提供用电，无天然气、煤气提供，具备冷藏保鲜（2-5℃）储存功能。\n7.设备尺寸（长高深）：约2100×2050×1000 (mm)。\n8.设备重量：约1500KG。",{"$nulls":7},"保修2年"]
[null,"人民币大写：",{"$nulls":6},{"$f":"SUM(I3:I3)","v":{"v":0,"d":"0.00"}}]
["备注：报价包含运输费、税费、安装调试费。售后服务按照国家三包规定执行，出现质量问题7日内可退换货‌，15日内换货或修理"]