{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":60,"n_cols":5,"rows_kept":60,"merged":[[0,0,0,4],[1,0,51,0],[57,0,62,0]]}
["新生儿防盗系统参数及配置情况表"]
["参数","序号","详细项目（▲代表实质性需求，★代表重要参数）","产品是否符合（是/否）","备注(若不符合请在此栏填写设备相应功能)"]
[null,1,"一、主要技术规格及系统参数"]
[null,2,"（一）蓝牙网关及蓝牙网关嵌入式软件："]
[null,3,"1.供电方式：两种供电方式，POE和DC 9~15V\n"]
[null,4,"2.终端接入数量：支持终端接入数量大于500个"]
[null,5,"3.接口：继电器开关并可输出12V电源，对接声光报警器"]
[null,6,"4.芯片：三芯片多核工作，在蓝牙跳频的基础上稳定接受每个广播通道的终端数据，确保信号不断连"]
[null,7,"5.蓝牙网关数量：23个"]
[null,8,"6.蓝牙网关嵌入式软件：23套"]
[null,9,"（二）护士/家长智能环及对应嵌入式软件"]
[null,10,"1.显示屏：OLED彩色显示屏"]
[null,11,"2.充电方式：USB充电"]
[null,12,"3.供电方式：可充电锂离子电池，电池容量≥130mah"]
[null,13,"4.护士/家长智能环数量：13个"]
[null,14,"5.护士/家长智能环嵌入式软件：13套"]
[null,15,"(三）监护智能环及对应嵌入式软件"]
[null,16,"1.使用频段：BLE 2.4G"]
[null,17,"2.OLED显示屏：约0.42寸"]
[null,18,"3.充电方式：磁吸式充电"]
[null,19,"4.防水级别：IPX8及以上防水功能"]
[null,20,"5.监护智能环数量：25个"]
[null,21,"6.监护智能环嵌入式软件：25套"]
[null,22,"7.监护智能环腕带≥100根，且尺寸多样化，大小规格满足医院需求；\n同时可实现断带报警"]
[null,23,"（四）婴儿防盗监控系统软件1套"]
[null,24,"1.婴儿防盗首页\n"]
[null,25,"2.实时监控"]
[null,26,"3.报警记录"]
[null,27,"4.病区工作站接入端口授权,每病区许可，数量：2套"]
[null,28,"（五）USB多口充电器"]
[null,29,"1.工作指示灯：1个"]
[null,30,"2.散热方式：风扇"]
[null,31,"3.充电数量终端：满足10个终端同时充电"]
[null,32,"4. 充电器数量：2个"]
[null,33,"（六）充电座"]
[null,34,"1.支持15个智能环同时充电\n"]
[null,35,"2.数量：2个\n"]
[null,36,"（七）频闪警示灯"]
[null,37,"1.数量：8个"]
[null,38,"2.颜色：红色"]
[null,39,"（八）高清摄像头"]
[null,40,"1.像素≥400万"]
[null,41,"2.分辨率≥1080P"]
[null,42,"3.DC 12V/POE"]
[null,43,"4.数量：8个"]
[null,44,"（九）其它"]
[null,45,"线缆材料：超六类及以上网线，≥360米"]
[null,46,"通信网络交换机：24 口百兆 poe 交换机，≥2个"]
[null,47,"二、其它："]
[null,48,"▲维保年限≥3年"]
[null,49,"▲配件维保过后只收成本费"]
[null,50,"▲服务年限过后维保费用不超过售价的10%，具体以实际谈判为准"]
[null,51,"▲总报价中包含HIS对接开发人工、安装、调试、研发等费用"]
[null,52]
[null,53]
[null,54]
[null,55]
["补充参数及配置\n\n（根据产品本身可自行补充，若无，可不填写）",56,null,"产品参数","备注"]
[null,57]
[null,58]